**Common Committee**

Vidyasagar Group of Colleges

39, Sankar Ghosh Lane

Kolkata-700006

**TENDER NOTICE FOR PAINTING & PLUMBING WORK AT PHYSICS LAB, GENTS AND LADIES TOILET IN VIDYASAGAR GROUP OF COLLEGES**

Tender No: VGC/PAINT & PLUMB/2023 -1 Date: 10.10.2023

Quotations are invited in sealed cover for Painting & Plumbing work at Physics lab, gents and ladies toilet in Vidyasagar Group of Colleges (old building) 39, Sankar Ghosh Lane Kolkata-700006 as per Annexure from established contractors with proven track record.

Vendors may visit the actual site during office hours i.e 11 am to 4p.m(Contact :9123318397)

Time limit of completion of the work 30 days after issuing of work order.

Interested vendors are requested to submit tender in sealed envelope containing quotation, copy of trade license, GST registration certificate, PAN card and Credentials(if any) *addressing to the*Convener, Common Committee, Vidyasagar Group of Colleges.The Common Committee of Vidyasagar Group of Colleges will not be liable for late receiving of any quotation. The Common Committee of Vidyasagar Group of Colleges has a right to reject any quotation without assigning any reason and the decision will be binding all.

**Important Notes:**

|  |  |  |  |
| --- | --- | --- | --- |
| 1. | Date of Publication of Tender | : | 10.10.2023 |
| 2. | Time for Submission | : | 11.00 am to 4.00 pm (except Holidays) |
| 3. | Last date for submission | : | 17.10.2023 upto 2.00pm |
| 4. | Place of Submission | : | Tender box placed at the first floor in front of room no. 9 of Vidyasagar College (old building) 39, Sankar Ghosh Lane Kolkata-700006 |
| 5. | Opening of Tender | : | 17.10.2023 at 2.15 pm |

 Sd/-

 Convener

 Common Committee

Vidyasagar Group of Colleges

**Annexure**

|  |
| --- |
| **Painting & Plumbing work at Physics lab, gents and ladies toilet in Vidyasagar Group of Colleges (Old Building)**  |
| **Sl. No.** | **Description of Items** | **Unit** | **Qnty.** | **Rate (Rs.)** | **Amount (Rs.)** |
| **1** |  **PAINTING**  |  |  |  |   |
| 1.1 | Priming one coat on timber or other plastered surface with Synthetic oil bound primer of approved quality including smoothening surface by sand papering etc. | Sq.M | 150.00 |   |   |
| 1.2 | Painting on timber surface with best quality synthetic enamel paint of approved make and brand including smoothening surface by sand papering etc. including using of approved putty etc. on the surface, if necessary.  | Sq.M | 50.00 |   |   |
| 1.3 | Applying Acrylic Emulsion Paint approved make and brand on walls and ceiling including sand papering in intermeadiate coats including putty. Two or more coats to give an even shade. Luxury Quality | Sq.M | 150.00 |   |   |
| 1.4 | (a) Priming one coat on steel or other metal surface with synthetic oil bound primer of approved quality including smoothening surfaces by sand papering etc. | Sq.M | 50.00 |   |   |
| 1.5 | Rendering the surface of walls, ceiling with white cement based wall putty of approved make and brand. (1.5mm thick).  | Sq.M | 150.00 |   |   |
| 1.6 | (A) Painting with best quality synthetic enamel paint of approved make and brand including smoothening surface by sand papering etc. including using of approved putty etc. on the surface, if necessary : **(a) On steel or metal surface : With super gloss (hi-gloss) - (iv) Two coats (with any shade except white)** | Sq.M | 50.00 |   |   |
| 1.7 | Scraping and removing greasy soot from walls or ceiling of kitchen or similar  | Sqm | 150.00 |   |   |
| **2** | **SANITARY AND PLUMBING WORKS** |   |   |   |   |
| 2.1 | Supply of UPVC pipes (B type) & fitting, fixing conforming to IS - 13592 - 1992. i) single socket 110mm. (S&P (B) (B) II It. No. 23Aib,24) | metre | 10.00 |   |   |
| 2.2 | Supplying, fitting and fixing CPVC (Chlorinated Polyvinyl Chloride) pipes of approved make conforming to IS-15778: 2007 . with all necessary accessories, specials viz. socket, bend, tee, union, cross, elbo, nipple, longscrew, reducing socket, reducing tee, short piece etc.fitted with holder bats clamps, including cutting pipes, fitting, fixing etc. complete in all respect including cost of all necessary fittings as required,jointing materials in any position above ground. (Payment will be made on the centre line measurements of total pipe line includingall specials. No separate payment will be made for accesories, specials. |   |   |   |   |
| i) | 15mm dia. Medium quality. | Mtr. | 25.00 |   |   |
| ii) | 20 mm dia. Medium quality. | Mtr. | 30.00 |   |   |
| iii) | 32 mm dia. Medium quality. | Mtr. | 10.00 |   |   |
| 2.3 | Supplying, fitting and fixing Peet's valve fullway gunmetal standard pattern best quality of approved brand bearing ISI marking with fitting (tested to 21Kg / sq.cm).  |   |   |   |   |
| i) | 25 mm. Dia.  | Each | 2.00 |   |   |
| ii) | 40 mm. Dia.  | Each | 1.00 |   |   |
| 2.4 | Supplying, fitting and fixing white vitreous china best quality approved make wash basin with C.I. brackets on 75 mm X 75 mm wooden blocks, C.P. waste fittings of 32 mm dia., one approved quality brass C.P. pillarcock of 15 mm dia., C.P. chain with rubber plug of 30 mm dia., approved quality P.V.C. waste pipe with C.P. nut 32 mm dia., 900 mm long approved quality P.V.C. connection pipe with heavy brass C.P. nut includingmending good all damages and painting the brackets with two coats of approved paint. (i) 450 mm X 300 mm size | Each | 2.00 |   |   |
| 2.5 | Supplying, fitting and fixing E.W.C. in white glazed vitreous chinaware ofapproved make complete in position with necessary bolts, nuts etc.(a) With 'P' trap  | Each | 2.00 |   |   |
| 2.6 | Supplying,fitting and fixing 32 mm dia. Flush Pipe of approved make withnecessary fixing materials and clamps complete.i) Polythene Flush Pipe  | Each | 2.00 |   |   |
| 2.7 | Supplying, fitting and fixing bevelled edged mirror 5.5 mm thick silver redas per I.S. 3438 / 1965 together with brass C.P. hinges.(i) 450 mm X 300 mm  | Each | 2.00 |   |   |
| 2.80 | Supplying, fitting and fixing 10 litre P.V.C. low-down cistern conforming toI.S. specification with P.V.C. fittings complete,C.I. brackets including twocoats of painting to bracket etc. | Each | 1.00 |   |   |
| 2.90 | Supplying,fitting and fixing approved brand P.V.C. CONNECTOR whiteflexible, with both ends coupling with heavy brass C.P. nut, 15 mm dia.450 mm long | Each | 10.00 |   |   |
| 2.10 | Supplying, fitting and fixing bib cock or stop cock. **(a)** (i) Chromium plated Bib Cock short body/ angular stop cock (Equivalent to Code No. 511 & Model - Tropical / Sumthing Special of ESSCO or similar brand). | Each | 8.00 |   |   |
| 2.11 | Supplying, fitting and fixing Flat back urinal (half stall urinal) in white vitreous chinaware of approved make in position with brass screws on 75 mm X 75 mm X 75 mm wooden blocks complete. (i) 635 mm X 395 mm X 420 mm each 2869.00 (ii) 470 mm X 280 mm X 340 m | Each | 3.00 |   |   |
| 2.12 | Supplying, fitting and fixing Squating plate with integral flushing in white vitreous chinaware of approved make in cement concrete (6:3:1) with jhama chips complete. (Payment of concrete will be paid seperately). (i) 450 mm X 350 mm | Each | 3.00 |   |   |
|   |   |   |   | **TOTAL** |  |
|  | GST @ 18%  |   |  |  |  |
|  |  |  |  |  |   |
|  |  |  | **Grand Total:** |  |
|  |  |  |  |  |  |
|  | (Rupees ……………………………………………………………………………………………….. ) |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  | Date: | Signature of the Contractor |
|  | Place: |  |  |  |  |